**2023 OSAGE *“2168 SUPER WARRIOR”* TYPE I**

**2023 FORD *“F-550”***

**STANDARD FEATURES**

**• MEMBER AMD / NTEA & FORD QVM PROGRAM •**

**• CERTIFIED KKK-1822-F & ALL REVISIONS •**

**• CERTIFIED CAAS GVS V2.0 •**

## CHASSIS

• 2023 Ford F-550 w/ 47A Amb Prep Pkg

• 193” Wheelbase w/ Dual Rear Wheels

• GVWR: 18,000 LBS

• 6.7 L Turbo Diesel w/ Ford Block Heater

• Ford Engine Hour Meter

• Ford Auxiliary Idler Control Unit

• Torqshift™ w/ SelectShift 10-Speed

 Automatic Transmission

• 4-Wheel Disc Brakes w/ ABS

• Stainless Steel Wheel Inserts

• Aluminum Diamond Plate Running Boards

• Rear Mud Flaps

• Dual Air Bags

• Dual Map Lights

• Tilt Steering Wheel & Cruise Control

• Electric Windows & Door Locks

• Keyless Remote Entry

• AM/FM Stereo Clock Radio w/ CD

• Deluxe Cloth High Back Captains Chairs

• Rubber Floor Mat I.L.O. Carpet

• Ford OEM Mirrors, Heated and Power Adjust

• Daytime Running Lights

* Choice of 2WD or 4WD

## MODULE

• Module Dimensions:

 168” L x 91” H x 96” W

• **Totally “Seamless” Body Construction**

• Exterior Side & Roof Panels .125” Aluminum

• One-Piece Exterior Side Panels

• One-Piece Crowned Roof

• Frame Members 2” x 2” Aluminum Tubing

• Frame Members on 12” Centers

• Diamond Plate Shields:

 \* Across Lower Rear of Body

 \* Across Lower Front of Body

 \* Lower 1/3 of Entry Doors

• All Exterior Doors “Pan-Formed” / Extruded

 Double Break Construction

• All Body Openings **“Seamless”**

• **All Door Latches Mounted Behind Gaskets**

• Exterior Compartment @ Front Left for

 Storage of Oxygen Tank and Back Boards

• Curbside Backboard Storage

• Exterior Compartment Adjustable Shelving

• Exterior Compartment LED Lighting

• Cast “Grabber” Door Holders

• Lower Body Impact Rub Rails

• Polished Stainless Steel Fenderettes

• Grip Strut Rear Step Bumper w/ Flip-up

 Center Section & 4” x 18” Dock Bumpers

• Automotive Undercoating

## WARNING SYSTEM

• Two Red Whelen 5x2 LED’s Mounted in Grill

• Two Red Whelen 5x2 LED Intersection Lights

 Mounted in Front Fenders

• Eight Red LED Whelen 9x7 Modular Lights

• One Clear LED Whelen 9x7 Front Center

• One Amber LED Whelen 9x7 Rear Center

• Two LED Whelen 9x7 Scene Lights per Side

• Two LED Whelen 9x7 Rear Load Lights

• Primary / Secondary Switching

• Carson SA 400 Siren w/ Siren / Horn Switch
• Cast Siren Speaker

• Rear DOT Lighting Whelen LED 4x6 w/

 Chrome Flanges: Red Tail / Brake,

 Amber Arrow Turn, Reverse

• LED Clearance / Marker Lights

## PAINT & MARKINGS

• 8” Belt Line Paint Stripe • “No Smoking” & “Fasten Seat Belt” Signs

• Base Coat / Clear Coat Modular Paint • Ambulance / Star-of-Life Decals

**2023 Osage *“2168 Super Warrior”* Type I - 2023 Ford *“F-550”* - Standard Features**

**ELECTRICAL**

• Ford OEM Dual Alternators, 397 Amps Total

• Digital Voltmeter

• Audible Low Voltage Alarm

• Bosch, Vanner, Cole-Herse & Weldon

 Components

• Weldon V-Mux 100% Solid State Micro-

 Processor Based Multiplex Electrical System

• Wiring Color-Coded and Heat Embossed

 Every 6” w/ Function

• Power Distribution Panel Easily Accessible

 Via Hinged Access Door in Action Area

• Front Switch Console Mounted on the Floor

• Hinge Mounted Attendant Switch Console

• Control Console Backlighting Dimmer

• Battery Switch Activated via Ignition Switch

• Open Door Warning Light

• Handheld LED Spotlight, Hardwired

• Whelen Dual Intensity LED Patient

 Compartment Dome Lights

• Exterior Weatherproof Shoreline Receptacle

• Two Interior 110V Duplex Receptacles

• Two Interior 12V Cigar Style Receptacles

• One Pre-Wire Antenna Cable

• Electrical Back-up Alarm w/ Auto Re-set

## INTERIOR

• 72” Interior Headroom

• 49” Aisle Width

• All Vertical Corners 1” Radii

• Stainless Steel Aisle Panel, Left Side,

 Full Length x 18” x .060”

• Lon-Plate non-skid Vinyl Flooring

 Rolled 3” Up Both Sides of Aisle

• EMT Seat, Pedestal Mounted

 DeluxeVinyl Captains Chair

• CPR Seat, Three Piece, Molded Cushions

• Squad Bench w/ Second Patient Capability

• All Seat Cushions Seamless

• Retractable Seat Belts for All Locations

• Handicap Style, 1 ½” Diameter, Full Length,

Stainless Steel Overhead Grab Rail.

This Rail shall be treated with Agion

Anti-Bacterial Coating.

• Handicap Style, 1 ½” Diameter, Stainless Steel

Door Pulls on Patient Compartment Doors. These Bars shall be treated with Agion

Anti-Bacterial Coating.

* Double entry step on curbside entry door

• Sliding “Pass-thru” Window between Cab

 and Patient Compartment

• Padded Bulk-Head Cabinet Doors

• Headliner Thermoplastic Sandwiched Between

 Two Sheets of Aluminum Finished in

 Semi-Gloss White

• ALS Compartment w/ In/Out Access

• 2 Adjustable & 1 Fixed Shelf in ALS

• R-29 Reflectix Insulation throughout Module

• Thermostatically Controlled Patient

 Compartment Heat & Cool System

• 3-Speed Manual Fan Control

• Rear Heat & Cool Unit Mounted Floor Level;

 \* Moisture Drains Directly Through Floor

 \* Short Coolant Circulation Distance

 \* Eliminates Vertical Circulation of Coolant

 \* Unit Easily Accessible for Maintenance

• Overhead Air Distribution w/ Floor Level Filtered Air Return for Optimum Circulation

• Two Recessed, Swing-up Dual IV Hangers

• “Zico” Retaining Bracket for Oxygen “M” Cyl

• Three “Ohio” Oxygen Outlets

* SSCOR Suction System
* Locking Sharps Container (Shipped Loose)

• Locking Drug Compartment

• Digital “Atomic” Digital Clock w/ Seconds

• Stryker “Performance Load” Cot Fastener

##  WARRANTY

 • Three Year / 36,000 Mile Product Conversion

• Five Year / 100,000 Mile Modular Paint

 • Seven Year / 72,000 Mile Electrical System

• Lifetime Modular Body Structure

**“ALL WARRANTIES NON-PRO-RATED”**

 NOTE: See Warranty Certificate for Details

**OSAGE AMBULANCE • P.O. BOX 718 • LINN, MO. 65051**

**800-822-3634 • FAX: 573-897-3113**

**www.osageambulances.com**